Ekos
Ekos is an advanced cross-platform (, , ) observatory control and automation tool with a particular focus on Astrophotography. It is based on a modular extensible framework to perform common astrophotography tasks. This includes highly accurate GOTOs using astrometry solver, ability to measure and correct polar alignment errors, auto-focus & auto-guide capabilities, and capture of single or stack of images with filter wheel support. Ekos is shipped with .
Ekos introductory video
Features:
Control your telescope, Camera (& DSLRs), filter wheel, focuser, guider, adaptive optics unit, and any INDI-compatible auxiliary device from Ekos.
Built-in native autoguiding with support for automatic dithering between exposures and support for Adaptive Optics devices in addition to traditional guiders.
Extremely accurate GOTOs using astrometry.net solver (both Online and Offline solvers supported).
Load & Slew: Load a FITS image, slew to solved coordinates, and center the mount on the exact image coordinates in order to get the same desired frame.
Measure & Correct Polar Alignment errors using astrometry.net solver.
Easy to use Polar Alignment Assistant tool. A very quick and reliable tool to polar align your German Equatorial Mount!
Capture and record video streams in SER format.
Completely automated scheduler to control all your observatory equipment, select the best targets for imaging given current conditions and constraints, monitor weather conditions, and capture your data while you are away!
Smart Dark Library: All your dark frames with different binning/temperature/frame settings are saved for future use. Ekos re-uses dark frames intelligently without taking unnecessary captures. You can configure how long you want to reuse all the dark frames.
Define multiple driver profiles for local and remote setups. Switch among them easily.
Auto and manual focus modes using Half-Flux-Radius (HFR) method.
Automated unattended meridian flip. Ekos performs post meridian flip alignment, calibration, focusing, and guiding to resume the capture session.
Automatic focus between exposures when a user-configurable HFR limit is exceeded.
Powerful sequence queue for batch capture of images with optional prefixes, timestamps, filter wheel selection, and much more!
Export and import sequence queue sets as Ekos Sequence Queue (.esq) files.
Center the telescope anywhere in a captured FITS image or any FITS with World Coordinate System (WCS) header.
Automatic flat field capture, just set the desired ADU and let Ekos does the rest!
Automatic abort and resumption of exposure tasks if guiding errors exceed a user-configurable value.
Support for dome slaving.
Complete integration with Observation Planner and SkyMap.
Fully scriptable via .
Integrate with all INDI native devices.